Geo Fence Config


[bookmark: _GoBack]1. Log in to the IVMS client and select Geo fence shapeIt will pop up a window and please add the name of the fence, click OK.
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2. Select the Terminal parameters and fill in the basic settings in the window shown as below.
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3. Select the Geo Fencing report
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