How to add the channel numbers

There are some situation about adding the channel number.

How to add the channel number of Monitor for example from 4 to 5.  
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Please use the remote control click the image as below.
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Then Select the “5 Screen “option of Live Mode.
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Finally, you can see there are five screen as below.
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Note: There is the FAQ about how to add IP camera.

https://www.icarvisions.com/faq/how-to-add-ip-camera-to-mdvr-226.html
How to add the channel number of IVMS Client and Mobile APP.

The default channel number of the vehicle are four.
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Please select the channel number for example “ 5 ” when you edit the vehicle info.
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After that, you will see there are five channels of the vehicle in IVMSClient

 and Icarview.
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